**Aluminium shower panel with SECURITHERM sequential mixer**

Sequential thermostatic mixer

Top fed, fixed shower head, aluminium, flexibles

Reference: **H9639**

Specification description

Anodised aluminium shower panel for wall-mounted exposed installation:

SECURITHERM sequential thermostatic mixer (non-time flow).

Adjustable temperature control from cold water up to 39°C; maximum temperature limiter set at 39°C, can be adjusted.

Anti-scalding failsafe: automatic shut-off if cold water supply fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation at 6 lpm at 3 bar.

Hygiene control lever L. 100mm.

Top inlets with inline M1/2" stopcocks.

Concealed fixings.

Filters.

Suitable for people with reduced mobility.

30-year warranty.