**TEMPOMATIC Electronic tap**

Mains supply

Cross wall 155mm

Reference: **441157**

Specification description

Cross wall electronic basin tap:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Chrome-plated fixed spout L. 170mm with anti-rotating pin and back-nut.

Plate is flush to wall.

Shockproof infrared presence detection sensor for wall ≤ 155mm

Anti-blocking security.

For walls ≤ 155mm.

Solenoid valve with integrated filter.

Threaded rods can be cut-to-size.

Suitable for people with reduced mobility.

30-year warranty.