**TEMPOMIX time flow mixer**

With stopcocks

Single control

Reference: **795000**

Specification description

Deck-mounted single control time flow basin mixer:

Soft-touch operation.

Temperature control and operation via the push-button.

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Chrome-plated solid brass body.

PEX flexibles with stopcocks F3/8", filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Adjustable maximum temperature limiter.

Ergonomic chrome-plated metal push-button.

30-year warranty.