**TEMPOMIX time flow mixer**

Cross wall 230mm

Reference: **795209**

Specification description

Cross wall single control time flow basin mixer:

Soft-touch operation.

Temperature control and operation via the push-button.

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Chrome-plated solid brass body M¾".

Filters and non-return valves.

Adjustable maximum temperature limiter.

Tamperproof cross wall control ≤ 220mm.

Tamperproof fixed cross wall spout ≤ 230mm.

System for fixing to the wall via anti-rotating pin, back-nut and connection clamp.

Threaded rods can be cut-to-size.

Chrome-plated metal control.

30-year warranty.