**TEMPOSOFT MIX time flow mixer**

Soft-touch operation

Standard temperature control

Reference: **742100**

Specification description

Deck-mounted time flow basin mixer:

 Soft-touch operation.

 Time flow ~7 seconds.

 Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

 Scale-resistant aerator.

 Chrome-plated solid brass body.

PEX flexibles F3/8" with filters and non-return valves".

Fixing reinforced by 2 stainless steel rods.

Side temperature control with standard lever and adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.