**TEMPOSOFT MIX 2 time flow mixer**

Soft-touch operation, stopcocks

Standard temperature control

Reference: **742500**

Specification description

Deck-mounted time flow basin mixer:

Soft-touch operation.

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated brass body.

PEX flexibles with stopcocks F3/8", filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Side temperature control with standard lever and adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.