**TEMPOMIX 2 time flow mixer**

(AB) Anti-blocking model

Standard temperature control

Reference: **700101**

Specification description

Deck-mounted time flow basin mixer:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Chrome-plated brass body.

PEX flexibles F3/8" with filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Side temperature control with standard lever and adjustable maximum temperature limiter.

AB anti-blocking system: water will flow only when the push-button is released

30-year warranty.