**TEMPOSTOP time flow tap**

(AB) Anti-blocking model

Wall-mounted with swivel spout, M½"

Reference: **748151**

Specification description

Wall-mounted time flow tap with swivel spout:

Time flow ~15 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated solid brass body M½".

Suitable for wash tubs.

AB anti-blocking system: water will flow only when the push-button is released.

30-year warranty.