**Fixed spout**

L.75mm

Cross wall 230mm

Reference: **942200**

Specification description

Spout L. 75 mm, M1/2".

For cross wall installation ≤ 230mm with anti-rotating pin.

Threaded rods can be cut-to-size.

Streamlined ligature-resistant design.

Chrome-plated solid brass.

Star-shaped scale-resistant flow straightener.

30-year warranty.