**Reinforced wall plate**

For TEMPOMIX, TEMPOSTOP or wall-mounted TEMPOSOFT

Ø 80mm, 4 screws

Reference: **824800**

Specification description

Wall plate or reinforcement for TEMPOSTOP or TEMPOMIX wall-mounted valve.

4 fixing screws.

F12 x 1,5.

4mm thick.

Recommended for installing on panel or dry wall.