**SECURITHERM shower panel**

Electronic battery-operated thermostatic

Concealed inlet,fixed head, aluminium

Reference: **792410**

Specification description

Electronic thermostatic shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

With concealed inlet via flexibles, M1/2".

SECURITHERM thermostatic mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Battery-operated with 223 6V Lithium battery.

Infrared presence detection. Shower starts when hand is 4cmfrom the sensor.

Shuts off on demand or automatically after ~60 seconds.

Duty flush (~60 seconds every 24 hours after the last use).

Flow rate set at 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

Concealed fixings.

Filters and non-return valves.

Suitable for people with reduced mobility.

30-year warranty.