**SECURITHERM shower panel**

Thermostatic time flow

Top inlet, fixed shower head, aluminum

Reference: **792300**

Specification description

Thermostatic time flow shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlet via in-line stopcocks M½".

SECURITHERM thermostatic shower mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Soft-touch operation.

Chrome-plated, tamperproof, scale-resistant fixed, ROUND shower head with automatic flow rate regulation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Concealed fixings.

Filters and non-return valves.

This product is compatible with thermal and chemical shocks in accordance with current guidelines.

Time flow shower panel suitable for people with reduced mobility.

30-year warranty.