**TEMPOMIX time flow shower panel**

Time flow single control

Top inlet, handset, aluminium

Reference: **790350**

Specification description

Time flow aluminium shower panel with handset:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlet supply with in-line stopcocks M½".

TEMPOMIX mixer with adjustable maximum temperature limiter.

Soft-touch operation.

Time flow ~30 seconds.

Sliding handset on chrome-plated rail with flexible hose.

Concealed fixings.

Filters and non-return valves.

30-year warranty.