**TEMPOMIX time flow shower kit**

Single control time flow

Recessed, ROUND head, st. steel plate 160x160mm

Reference: **790709**

Specification description

Recessed time flow shower kit:

Stainless steel wall plate 160 x 160mm.

Standard recessing housing.

Recessing depth can be adjusted from 28 to 48mm.

TEMPOMIX ¾" single control mixer.

Ligature-resistant collar.

Temperature control and operation via the push-button.

Maximum temperature limiter (can be adjusted by the installer).

Time flow ~30 seconds, soft-touch operation.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

M½" connections for copper tubes Ø 14mm.

Integrated non-return valves and filters.

Chrome-plated metal control.

30-year warranty.

This model does not have a waterproof recessing box. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).