**TEMPOMIX time flow shower kit**

Single control time flow

Cross wall 220mm, mixer, ROUND shower head

Reference: **796209**

Specification description

Time flow shower kit for cross wall installation:

TEMPOMIX ¾" single control mixer.

For walls ≤ 220mm.

Temperature control and operation via the push-button.

Maximum temperature limiter (adjustable by the installer).

Ligature-resistant collar.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated ROUND shower head, tamperproof with scale-resistant nozzle and automatic flow rate regulation.

Integrated non-return valves and filters.

Chrome-plated metal push-button.

Integrated non-return valves and filters.

Threaded rods can be cut-to-size.

30-year warranty.