**TEMPOMIX time flow shower kit**

Single control time flow

TONIC JET shower head, mixer, elbow STOP unions

Reference: **790006**

Specification description

Time flow shower kit for exposed installation:

TEMPOMIX ¾" single control mixer.

Wall-mounted installation.

Temperature control and operation via the push-button.

Maximum temperature limiter (can be adjusted by the installer).

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant TONIC JET shower head with automatic flow rate regulation.

Chrome-plated solid brass.

Integrated non-return valves and filters.

Chrome-plated metal push-button.

Shower column Ø 16mm and collar (mounting bracket and screws supplied).

Elbow M½" STOP unions, 150mm centres.

30-year warranty.