**TEMPOSOFT 2 time flow shower valve**

Time flow

Exposed, angled, soft-touch operation

Reference: **748800**

Specification description

Time flow shower valve for exposed installation:

TEMPOSOFT 2 M½" time flow valve for mixed water supply.

For wall-mounted installation.

Angled for recessed inlet.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate pre-set at 6 lpm at 3 bar, can be adjusted.

Chrome-plated solid brass body.

Suitable for people with reduced mobility.

30-year warranty.