**TEMPOSTOP time flow shower valve**

Time flow

Recessed, st steel wall plate Ø 130mm

Reference: **749128**

Specification description

Recessed time flow shower valve:

TEMPOSTOP F1/2" time flow valve for mixed water supply.

For recessed installation.

Stainless steel wall plate Ø 130mm.

Recessing depth between 25 to 40mm .

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar, can be adjusted.

Chrome-plated brass body and button.

30-year warranty.

This model does not have a waterproof recessing box. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).