**TEMPOSTOP time flow shower valve**

Time flow

Exposed, without flow rate regulator, M3/4"

Reference: **749000**

Specification description

Time flow shower valve for exposed installation:

TEMPOSTOP M¾" time flow valve for in-line mixed water supply.

For wall-mounted exposed installation.

Time flow ~30 seconds.

Flow rate 67 lpm at 3 bar.

Chrome-plated solid brass body and push-button.

30-year warranty.