**TEMPOSTOP time flow shower valve**

Time flow

Exposed, angled, M1/2"

Reference: **748000**

Specification description

Time flow shower valve for exposed installation:

TEMPOSTOP M1/2" time flow valve for mixed water supply.

For wall-mounted exposed installation.

Angled for recessed inlet.

Time flow ~15 seconds.

Flow rate pre-set at 9 lpm at 3 bar, can be adjusted.

Chrome-plated solid brass body and push-button.

30-year warranty.