**ROUND shower head**

Scale-resistant

Cross wall 230mm

Reference: **709200**

Specification description

Fixed shower head:

For cross wall installation (230mm max.).

Cut-to-size threaded rod.

Flow rate 6 lpm at 3 bar.

Automatic flow rate regulation.

Scale-resistant and ligature-resistant adjustable nozzle.

Chrome-plated brass.

Fixed with concealed blocking screw.

Systematically drains after use (no water retention or impurity deposits).

Inlet M½".

30-year warranty.