**PREMIX NANO thermostatic mixing valve**

For mixed water from 34 - 60°C

Nickel-plated body, inlets F3/8" and outlet M3/8"

Reference: **732012**

Specification description

Thermostatic mixing valve for mixed water distribution from 34 - 60°C:

 For 1 to 2 taps or 1 shower.

 Anti-scalding safety: automatic water shut-off in case of hot or cold water supply failure.

 Temperature pre-set at 38°C, can be adjusted by the installer from 34 - 60°C.

 Non-return valves and filters.

 Minimum flow rate for operation: 3 lpm.

 Thermal shocks are possible.

 Nickel-plated body, inlets F3/8" and outlet M3/8".

30-year warranty.