**Deck-mounted single hole mixer - 20 lpm**

Swivelling tubular over spout L. 300mm H. 315mm

Slimline control lever

Reference: **2506T3**

Specification description

Deck-mounted single hole mixer with swivelling, tubular spout H. 315mm L. 300mm.

Star-shaped flow straightener.

Ceramic cartridge Ø 35mm.

Flow rate 20 lpm at 3 bar.

Spout with smooth interior.

Slimline control lever.

Chrome-plated body and spout with reinforced fixing via two stainless steel rods and back-nuts.

Without pop-up waste.

Supplied with stainless steel braided PEX flexibles F3/8".

30-year warranty.