**Deck-mounted single hole mixer - 45 lpm**

Swivelling over spout L. 200mm H. 195mm

Reference: **5640T2**

Specification description

Deck-mounted single hole mixer with swivelling, tubular spout Ø 22mm H. 195mm L. 200mm.

Star-shaped flow straightener.

Water-free, guided valve heads with reinforced mechanisms.

Shock-resistant, ergonomic ball levers.

Flow rate 45 lpm at 3 bar.

Full flow rate achieved within first 90°.

Spout with smooth interior.

Chrome-plated brass body and spout.

Reinforced fixing via two stainless steel rods.

F3/8" PEX flexibles.

30-year warranty.