**Deck-mounted single hole mixer - 45 lpm**

Swivelling over spout H. 190mm L. 300mm

Reference: **5640T3**

Specification description

Deck-mounted single hole mixer with swivelling, tubular spout Ø 22mm H. 190mm L. 300mm.

Star-shaped flow straightener with smooth interior.

Water-free, guided valve heads with reinforced mechanisms.

Shock-resistant, ergonomic ball levers.

Flow rate 45 lpm at 3 bar.

Full flow rate achieved within first 90°.

Chrome-plated brass body and spout.

F3/8" PEX flexibles.

Reinforced fixings via two stainless steel rods.

Mixer suitable for intensive use in professional kitchens.

Mixer with 30-year warranty.