**Wall-mounted twin hole mixer - 30 lpm**

Telescopic spout L. 200 - 290mm

Reference: **G6679**

Specification description

Wall-mounted twin hole mixer with telescopic, swivelling spout Ø 22mm L. 200 - 290mm.

Star-shaped flow straightener.

Water-free, guided valve heads with control knobs.

Flow rate 30 lpm at 3 bar.

Chrome-plated brass body and spout.

Mixer can be installed with the spout above or below.

Wall connectors not included.

30-year warranty.