**Eye wash station**

Deck-mounted - single spray

Trigger-operated

Reference: **9140C**

Specification description

Deck-mounted single spray eye wash with:

Eye wash spray head with protective cap in green ABS; will eject automatically when activated.

Press the trigger to operate eye wash spray.

A spring automatically shuts off spray.

Flow rate 6 lpm at 3 bar. Aerator with stainless steel double filter.

Ergonomic grip and trigger in green polypropylene.

Supplied with identification sign for first aid equipment "Eye Wash".

Spray head with flexible hose L. 1.50m, 15 x 100, 1/2".

30-year warranty.