**Twin hole pre-rinse set with mixer**

Without bib tap

White flexible and scale-resistant hand spray

Reference: **G6533**

Specification description

Complete pre-rinse set without bib tap suitable for intensive use in professional kitchens.

Deck-mounted twin hole mixer with adjustable centres 100 - 240mm with:

- valve heads with control knobs.

- offset inlet connections with M1/2" tails.

- supplied with non-return valves.

White hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433000).

Scale-resistant hand spray with shock-resistant tip.

White, reinforced, food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.

These pre-rinse sets can be installed close to the splashback.