**Twin hole pre-rinse set with mixer**

Without bib tap

Black flexible and scale-resistant hand spray

Reference: **5680**

Specification description

Complete pre-rinse set without bib tap suitable for intensive use in professional kitchens.

Deck-mounted twin hole mixer with 150mm centres with:

- valve heads with reinforced mechanisms with ergonomic control levers.

- offset inlet connections with M1/2" tails.

Black hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433010).

Scale-resistant hand spray and shock-resistant tip.

Black reinforced, food-grade flexible hose L. 0.95m.

3/4" stainless steel column.

Adjustable wall bracket.

Stainless steel spring guide.

Twin hole pre-rinse set with 30-year warranty.

These pre-rinse models can be installed close to the splashback.