**Wall-mtd shower-bath mixer**

Mechanical shower mixer with sculptured control lever

With offset standard connectors

Reference: **2252S**

Specification description

Mechanical shower-bath mixer.

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.

Fitted with and automatic diverter with low pressure lock to maintain the shower position even if the flow rate is too low.

High sculptured control lever.

M1/2" shower outlet with integrated non-return valve.

Chrome-plated brass body.

Mixer supplied with offset standard connectors, M1/2" M3/4".

30-year warranty.