**TEMPOSOFT MIX time flow mixer**

Soft-touch operation, stopcocks

Long temperature control lever

Reference: **742000LH**

Specification description

Deck-mounted time flow basin mixer:

Soft-touch operation.

Time flow 7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant aerator.

Solid chrome-plated brass body.

PEX flexibles F3/8" with stopcocks, filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Side temperature control with long lever and adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.