**SECURITHERM shower panel**

Thermostatic time flow

Top inlet, fixed head, alu, soap dish

Reference: **792305**

Specification description

Thermostatic time flow shower panel:

Anodised aluminium shower panel for wall-mouted, exposed installation.

With top inlet via in-line stopcocks M1/2".

SECURITHERM thermostatic mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate set at 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

With soap dish.

Concealed fixings.

Filters and non-return valves.

Suitable for people with reduced mobility.

30-year warranty.