**TEMPOMIX time flow shower mixer**

Single control time flow

Chrome-plated Bayblend® control, elbow unions

Reference: **790874**

Specification description

Time flow shower mixer for exposed installation:

TEMPOMIX ¾" single control mixer.

For wall-mounted installation.

Temperature control and operation via the push-button.

Maximum temperature limiter (adjustable by the installer).

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar, can be adjusted.

Chrome-plated solid brass body.

Integrated non-return valves and filters.

Chrome-plated metal push-button.

Elbow unions, 150mm centres.

30-year warranty.