**TEMPOMATIC shower panel**

Electronic

Top inlet, fixed head, aluminum

Reference: **452300**

Specification description

Electronic shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

With top inlet via in-line stopcock, M1/2".

TEMPOMATIC electronic mixer for mixed water supply.

Battery-operated with 223 6V Lithium battery.

Infrared presence detection. Shower starts when hand is at 4cm from the sensor.

Shuts off on demand or automatically after ~60 seconds.

Duty flush (~60 seconds every 24 hours after the last use).

Flow rate set at 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

Concealed fixings.

Filter.

Suitable for people with reduced mobility.

30-year warranty.