**TEMPOMIX time flow shower panel**

Time flow single control

Concealed inlet, fixed head, st steel, soap dish

Reference: **790214**

Specification description

Time flow shower panel with fixed shower head:

Large model satin stainless steel panel for wall-mounted, exposed installation.

Concealed inlet via flexibles M½".

TEMPOMIX shower mixer with adjustable maximum temperature limiter.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation.

Integrated soap dish.

Concealed fixings.

Filters and non-return valves.

Stopcocks.

Shower panel suitable for people with reduced mobility.

30-year warranty.