**Wall-mounted MINERALCAST wash trough**

MINERALCAST - 3 services - L. 1800mm

With Ø 35mm central tap hole

Reference: **454182**

Specification description

Wall-mounted wash trough for wall-mounting, for 3 services.

MINERALCAST: composite material consisting of natural minerals and polyester resin.

Ideal for use in public and commercial places.

Uniform, non-porous surface is easy to clean.

One-piece cast washbasin, seam-free, for easy maintenance and better hygiene.

Pleasant to the touch.

With Ø 35mm central tap hole.

Supplied with 1½" waste. Without overflow.

Supplied with fixing elements.

White, RAL 9016.

CE marked. Complies with European standard EN 14296.

Weight: 90kg.

MINERALCAST pedestals in anthracite also available, sold individually (454001A or 454010).

30-year warranty.