**Tilting mirror with tab handle**

Bright white HR Nylon handle

Reference: **510202N**

Specification description

Wall-mounted, rectangular, tilting mirror with handle for easy adjustment by those in a seated position or in a wheelchair.

For disabled washrooms and combined installation: can be used from a sitting position, for people with reduced mobility, or standing position.

NylonClean lever with anti-bacterial treatment: optimal protection against bacterial development.

Quick and easy installation: just clip into place.

Anti-theft locking.

Tilting mirror with bright white HR Nylon handle.

6mm thick safety glass mirror.

Mirror dimensions: 500 x 600mm.

Can be tilted up to 20°.

Tilting mirror with 30-year warranty.