**Wall mounted MINERALCAST PMR washbasin**

MINERALCAST - 1 basin

With Ø 35mm central tap hole

Reference: **132306**

Specification description

Wall-mounted washbasin, 785 x 545 x 170mm.

With integral side grips, can be used to support user or as a towel rail.

Sleek and fluid lines.

MINERALCAST: a composite material consisting of natural minerals and polyester resin.

Suitable for use in public and commercial places and the healthcare sector.

Shallow washbasin ideal for people with reduced mobility.

Uniform, non-porous surface is easy to clean.

One-piece pressed washbasin, seam-free, for easy maintenance and better hygiene.

Warm to the touch.

With Ø 35mm central tap hole.

Without overflow.

Supplied with fixing elements.

White, RAL 9016.

CE marked. Complies with European standard EN 14688.

Weight: 21.5 kg.

30-year warranty.