**BIOSAFE mechanical basin mixer**

Single hole mechanical mixer with no spout, H. 95mm L. 110mm

With pop-up waste

Reference: **2620**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mechanical mixer H. 95mm L. 110mm.

No spout: BIOSAFE hygienic outlet integrated into the body.

Securitouch thermal insulation prevents burns.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Thermal shocks are possible without removing the control lever or shutting off the cold water supply.

Body with smooth interior and very low water volume (reduces bacterial development).

Flow rate regulated at 5 lpm.

Solid control lever.

Ergonomic pop-up waste 1 1/4" in brass.

PEX flexibles F3/8" with rotating unions.

Fixing reinforced by two stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Suitable for people with reduced mobility.

Mixer with 30-year warranty.