**TEMPOMIX 3 time flow shower mixer**

Time flow single control

Exposed, top outlet, soft-touch operation

Reference: **794400**

Specification description

Exposed time flow shower mixer:

TEMPOMIX 3 single control mixer, top outlet M¾".

For wall-mounted, exposed installation.

Temperature control and operation via the push-button.

Maximum temperature limiter (can be adjusted by the installer).

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar, can be adjusted from 6 - 12 lpm.

Chrome-plated brass.

Integrated filters and non-return valves.

Chrome-plated metal push-button.

M½" offset connectors for 130 - 170mm centres.

Suitable for people with reduced mobility.

30-year warranty.