**Bright polished stainless steel double coat hook**

Bright polished 304 stainless steel

Reference: **4042P**

Specification description

Double coat hook.

Wall-mounted coat hook.

Bacteriostatic bright polished 304 stainless steel.

Concealed fixings.

Tube Ø 20mm, 1mm thick.

Dimensions: Ø 62 x55 x 95mm.

30-year warranty.