**SECURITHERM Securitouch thermostatic shower mixer**

Dual control thermostatic shower mixer

With in-line STOP/CHECK connectors

Reference: **H9741TP**

Specification description

Dual control SECURITHERM thermostatic shower mixer.

Mixer with anti-scalding safety: shuts off automatically if cold water fails.

Prevents cold showers if hot water supply fails.

Securitouch thermal insulation to prevent burns.

Scale-resistant thermostatic cartridge for temperature adjustment.

¼-turn ceramic head for flow rate adjustment.

Temperature adjusts from 25°C to 41°C.

Maximum temperature limiter pre-set to 38°C.

Thermal shocks are easy to undertake without shutting off the cold water.

Flow rate regulated at 9 lpm.

Chrome-plated brass body and ERGO controls.

M1/2" shower outlet.

Filters and non-return valves built-in to inlets F3/4".

Mixer with inline STOP/CHECK connectors M1/2" M3/4".

Mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.