**SECURITHERM BIOCLIP thermostatic sink mixer**

Wall-mounted sequential thermostatic mixer

Offset STOP/CHECK unions, removable brass spout

Reference: **H9614P**

Specification description

Wall-mounted SECURITHERM thermostatic sink mixer.

Thermostatic sequential mixer: opens and closes with cold water.

No risk of cross flow between hot and cold water.

No non-return valves on the inlets.

Wall-mounted mixer supplied with 2 removable chrome-plated brass spouts L. 126mm.

Anti-scalding failsafe: shuts off automatically if cold or hot water supply fails.

Securitouch thermal insulation prevents burns.

Scale-resistant sequential thermostatic cartridge for sequential control of flow rate and temperature.

Temperature can be adjusted from cold water up to 40°C with temperature limiter set at 40°C.

Tested without water to meet NHS requirements. No preset temperature.

Thermal or chemical shocks are possible.

Body and spout with smooth interiors and low water volume.

Flow rate regulated at 7 lpm.

Chrome-plated brass body.

No manual contact thanks to Hygiene control lever L. 146mm.

Mixer with 200mm centres, supplied with 2 offset STOP/CHECK M1/2" M3/4" connectors ideal for hospitals.

Thermostatic mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Suitable for people with reduced mobility.

Mixer with 30-year warranty.