**TEMPOMIX 2 time flow mixer**

Ø 15mm stopcocks

Lever-operated, Standard temperature control

Reference: **70040015**

Specification description

Deck-mounted time flow basin tap:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated solid brass body

PEX flexibles with stopcocks, filters, non-return valves and Ø 15mm conical inlets.

Fixing reinforced by 2 stainless steel rods.

Side temperature control with standard lever and maximum temperature limiter.

Lever control (soft-touch operation).

30-year warranty.