**BINOPTIC electronic tap**

Battery-operated, Ø 15mm conical inlet

Spout with smooth interior

Reference: **47801515**

Specification description

Deck-mounted electronic basin tap:

Independent IP65 electronic control unit.

123 6V Lithium battery.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Active, infrared movement detection, sensor at the end of the spout optimises detection.

Chrome-plated solid brass body.

PEX flexible with filter, solenoid valve and Ø 15mm conical inlet.

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Spout with a smooth interior and low volume of water (limits bacterial niches).

Suitable for people with reduced mobility.

30-year warranty.