**TEMPOMATIC MIX PRO electronic mixer**

Mains supply, Ø 15mm conical inlets

Swivelling removable spout with smooth interior

Reference: **49525315**

Specification description

Deck-mounted electronic basin mixer:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 4 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Solenoid valves are upstream of the mixing chamber.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Shock-resistant infrared presence detection sensor.

Chrome-plated solid brass body with fixing reinforced by 2 stainless steel rods.

PEX flexibles with filters and solenoid valves Ø 15mm for compression fitting.

360° swivelling spout with smooth interior (reduces bacterial development).

Removable spout for cleaning.

Anti-blocking security.

Side temperature control with adjustable maximum temperature limiter and long ergonomic lever.

30-year warranty.

Two shut-off options:

Standard mode: timed flow with automatic shut-off

ON/OFF mode: user shuts off voluntarily or automatic shut-off after 30 minutes of flow. Thermal shocks are possible.