**TEMPOMIX 3 time flow mixer**

Soft-touch operation

Single control, Wall-mounted with fixed spout

Reference: **794360**

Specification description

Wall-mounted single control time flow basin mixer:

Soft-touch operation.

Temperature control and operation via the push-button.

Time flow pre-set at ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Chrome-plated metal body M½".

Fixed spout L.150mm.

Filters and non-return valves.

Adjustable maximum temperature limiter.

M½" offset connectors for centres from 130 - 170mm.

Suitable for people with reduced mobility.

30-year warranty.