**Lift-up Comfort shower seat with backrest and leg**

Wall-mounted lift-up shower seat

UltraSatin polished satin stainless steel

Reference: **510436S**

Specification description

HR Comfort lift-up shower seat with leg and backrest.

Shower seat for disabled people and for people with reduced mobility.

Wall-mounted lift-up shower seat and backrest for fixed installation.

Large model.

Anti-bacterial treatment on seat and backrest: optimal protection against bacterial development and mould.

Retained in upright position. Slowed down descent.

Suitable for intensive use in public places or the healthcare sector.

Removable solid seat and backrest made from high strength polymer.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products (Betadine®) and cleaning.

Anti-UV treatment.

Warm to the touch.

Bacteriostatic 304 stainless steel structure Ø 32mm.

UltraSatin polished satin finish stainless steel.

Reinforced by a folding, articulated leg made from 304 stainless steel tube Ø 25mm.

Concealed fixings secured to wall by a 304 stainless steel plate, 4mm thick.

Supplied with stainless steel screws for concrete walls.

Dimensions: 506 x 420 x 1,000mm.

Folded dimensions: 165 x 620mm.

Tested to over 250kg. Maximum recommended user weight: 170kg.

Lift-up shower seat and backrest with 30-year warranty. CE marked.