**TEMPOSTOP shower valve**

Time flow

Exposed, flow rate regulator, M3/4" M1/2'' Ø 15mm

Reference: **749721**

Specification description

Time flow shower valve for exposed installation:

TEMPOSTOP M3/4"-M1/2'' time flow valve for mixed water supply.

For wall-mounted installation.

Ø 15mm conical inlet.

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar with flow rate regulation.

Chrome-plated solid brass body and push-button.

30-year warranty.