**Adjustable height floor trap**

For tiles or concrete floors

150x150mm

Reference: **683001UK**

Specification description

Floor trap for hard floors (tiles or concrete) with adjustable height:

Flow rate 36 lpm (meets standards).

Water level 50mm.

Bright polished stainless steel plate and grid 150x150mm.

Ø 43mm horizontal outlet integrated into the height of the floor trap (saves height and space in all directions).

Integrated waterproof collar to seal waterproof membrane.

Withstands high temperatures: 60°C continuous, 85°C peak.

Plunger with handle: easy to grip and easy cleaning.

Smooth PVC body (prevents build-up of impurities).

Classified non-flammable (American certification UL94).

110mm high, adjusts up to 70mm with extension.

Grill fixed with two stainless steel screws.

30-year warranty.